

Welcome to use our IPC product.

Following is quick guide for CMS Software.



C:\Users\Administrator\AppData\Roaming\Tencent\Users\2261966921\QQ\WinTemp\RichOle\3FMNK1F{PPP`RS7(KR$B`N1.jpgclick CMS icon enter into CMS management software




Default User Name:super password:none




Above photo is main interface



Above photos are “PTZ”,“System” interface

C:\Users\Administrator\AppData\Roaming\Tencent\Users\604788781\QQ\WinTemp\RichOle\C$9UXOLP4}LG1UP8SMV3((O.jpgclick this icon to enter into “Device Manager”

Step 1:click “ADD AREA” to add zone, then add device




Step 2:“ADD DEVICE”-“IP Search” to Search out IP address-OK

Note:default User Name:admin password:none




Click “EditDevice” to update IP address and port



Cloud is P2P mode, input Serial ID to view

Note:default User Name:admin password:none

C:\Users\Administrator\Desktop\3PQ_PYTQ~LT]TT61)U@0][1.jpgclick this icon to enter into “Local Config”



Set Language for CMS software(20 language for choice):

Arabic,Chinese,Dutch,English,French,Finnish,Hebrew,Hungarian,Italian,Japanese,Korean,Polish,Portuguese,Romanian,Russian, Spanish, Traditional Chinese,Turkish….

C:\Users\Administrator\Desktop\BF$)TPD(T4R8]7UR(7$00QN.jpgclick this icon to enter into “Remote Config”



For Remote configure, please refer to IE Quick Manual